/*###ICF### Section handled by ICF editor, don't touch! ****/
/*-Editor annotation file-*/
/* IcfEditorFile="$TOOLKIT_DIR$\config\ide\IcfEditor\a_v1_0.xml" */
/*-Vector table start*/
define symbol __ICFEDIT_vector_start__ = 0x00400000;
/*-Memory Regions-*/
define symbol __ICFEDIT_region_RAM_start__  = 0x20000000;
define symbol __ICFEDIT_region_RAM_end__    = 0x20005FFF;
define symbol __ICFEDIT_region_ROM_start__  = 0x00400000;
define symbol __ICFEDIT_region_ROM_end__    = 0x0043FFFF;
/*-Sizes-*/
define symbol __ICFEDIT_size_cstack__        = 0x800;
define symbol __ICFEDIT_size_heap__          = 0x800;
/**** End of ICF editor section. ###ICF###*/

/* we place the stack at the end of RAM region */
define symbol __cstack_start__ = __ICFEDIT_region_RAM_end__+1-__ICFEDIT_size_cstack__;
export symbol __cstack_start__;
define symbol __cstack_end__ = __cstack_start__+__ICFEDIT_size_cstack__-1;
export symbol __cstack_end__;

define memory mem with size = 4G;
define region RAM_region = mem:[from __ICFEDIT_region_RAM_start__ to __ICFEDIT_region_RAM_end__] - 
                           mem:[from __cstack_start__ to __cstack_end__];
define region ROM_region = mem:[from __ICFEDIT_region_ROM_start__ to __ICFEDIT_region_ROM_end__];

define block CSTACK with alignment = 8, size = __ICFEDIT_size_cstack__ { };
define block HEAP with alignment = 8, size = __ICFEDIT_size_heap__ { };

initialize by copy with packing=none { readwrite };
do not initialize { section .noinit };

place at address mem:__ICFEDIT_vector_start__ { readonly section .intvec };
place in ROM_region { readonly };
place in RAM_region { readwrite, block HEAP };
place at address mem:__cstack_start__ { block CSTACK };
